Product Information / Technical Specifications

# Printer

> General
> Environmental
> Standards and approvals
> Mechanical
> Electrical
> PostScript

## General

Printing method: | Laser beam scanning and dry electrophotographic process
Resolution: | EPL-6200: 1200 dpi, Class 1200 dpi, or 600 dpi, 300 dpi EPL-6200L: 600 dpi
Printing speed: | 300dpi/600 dpi: | Up to 20 pages per minute with A4 paper
1200 dpi: | Up to 10 pages per minute with A4 paper
(depending on the font and data quantity)
First print: | Less than 13 seconds with A4/Letter paper (When feeding from MP tray at 600 dpi)
Paper feed: | EPL-6200: Automatic or manual feed EPL-6200L: Automatic
Paper feed alignment: | Center alignment for all sizes
Input paper supply (75 g/m2 paper): | MP tray: | EPL-6200: Up to 250 sheets of plain paper EPL-6200L: Up to 150 sheets of plain paper Up to 10 envelopes, depending on thickness
Paper output: | Face-down
Paper output capacity (75 g/m2 paper): | Up to 100 sheets of plain paper
RAM: | EPL-6200: 8 MB, expandable up to 136 MB EPL-6200L: 2 MB

[Top]

## Environmental

Temperature: | Operation: Storage: | 10 to 35°C (50 to 95°F) 0 to 35°C (32 to 95°F)
Humidity: | Operation: Storage: | 15 to 85% RH 30 to 85% RH
Altitude: | 2,500 meters (8,200 feet) maximum

[Top]

## Standards and approvals

Safety standards:

U.S. model: | UL 60950 CSA C22.2 No.60950
European model: | Directive 73/23/EEC EN60950

EMC:

U.S. model: | FCC part 15 subpart B class B
European model: | Directive 89/336 /EEC
| EN 55022 (CISPR Pub. 22) class B EN 55024 EN 61000-3-2 EN 61000-3-3
Australian model: | AS/NZS 3548 class B

[Top]

## Mechanical

Dimensions and weight: | EPL-6200: | Height: 261 mm (10.4 in.) Width: 407 mm (16.3 in.) Depth: 436 mm (17.4 in.) Weight: Approx. 7.5 kg (16.5 lb), excluding the developer cartridge and photoconductor unit
EPL-6200L: | Height: 261 mm (10.4 in.) Width: 385 mm (15.4 in.) Depth: 279 mm (11.1 in.) Weight: Approx. 7.5 kg (16.5 lb), excluding the developer cartridge and photoconductor unit
Durability: | 5 years or 180,000 sheets, whichever comes first

[Top]

## Electrical

### EPL-6200

| 110 to 120 V Model | 220 to 240 V Model
Voltage | 110 V - 120 V ± 10% | 220 V - 240 V ± 10%
Rated frequency | 50 Hz - 60 Hz ± 3 Hz | 50 Hz - 60 Hz ± 3 Hz
Rated current | 8.0 A | 4.5 A
Power consumption | During printing | Maximum | 900 W | 861 W
Average | 370 Wh | 372 Wh
Average during standby mode* | 44 Wh | 48 Wh
Sleep mode | Less than 7 Wh | Less than 7 Wh

### EPL-6200L

| 110 to 120 V Model | 220 to 240 V Model
Voltage | 110 V - 120 V ± 10% | 220 V - 240 V ± 10%
Rated frequency | 50 Hz - 60 Hz ± 3 Hz | 50 Hz - 60 Hz ± 3 Hz
Rated current | 8.0 A | 4.5 A
Power consumption | During printing | Maximum | 900 W | 825 W
Average | 372 Wh | 357 Wh
Average during standby mode* | 46 Wh | 48 Wh
Sleep mode | Less than 8 Wh | Less than 8 Wh

| * When no options are installed.

| Note:

Check the label on the back of the printer for the voltage of your printer.

### Laser safety

This printer is certified as a Class 1 laser product under the U.S. Department of Health and Human Services (DHHS) Radiation Performance Standard according to the Radiation Control for Health and Safety Act of 1968. This means that the printer does not produce hazardous laser radiation.

Since radiation emitted by the laser is completely confined within protective housings and external covers, the laser beam cannot escape from the machine during any phase of user operation.

### CDRH regulations

The Center for Devices and Radiological Health (CDRH) of the U.S. Food and Drug Administration implemented regulations for laser products on August 2, 1976. Compliance is mandatory for products marketed in the United States. The label shown below indicates compliance with the CDRH regulations and must be attached to laser products marketed in the United States.

[Top]

## PostScript

### Language

Adobe PostScript 3

### Emulation name

in PJL: | POSTSCRIPT
in EJL: | PS

### AppleTalk protocol

Entity Type: | LaserWriter
Emulation Type: | POSTSCRIPT-00

### Hardware requirements

Your printer must meet the following hardware requirements to be able to use the PostScript 3 printer driver.

- Memory requirements for using the PostScript 3 printer driver are shown below. Install optional memory modules into your printer if the amount of memory currently installed does not meet your printing needs.

Minimum memory | Recommended memory
8 MB* (for a simple print job at 300 dpi) | 40 MB or more

| * Printing may not be possible with this amount of memory, depending on the specifics of the job being printed.

[Top]

Previous | Next