Setup & Maintenance / Cleaning and Transporting the Printer

# Transporting the Printer

If you need to transport your printer, carefully repack it using the original box and packing materials as follows:

| Turn off the printer.

| Unplug the power cord from the electrical outlet and then from the printer.

| Disconnect all interface cables from the printer.

| Remove all paper from the MP tray.

| Remove or close the MP tray, depending on your printer model.

> EPL-6200

> Grasp the base part of the MP tray with both hands, pull the bottom edge outward, and pull it out of the printer.

> EPL-6200L

| Remove the optional 500-Sheet Lower Paper Cassette Unit A4 and/or Duplex Unit, if installed. (EPL-6200 only)

| Replace the printer's protective materials, then repack the printer in its original box.

|  | Caution:

Do not expose the photoconductor unit and the developer cartridge to light any longer than necessary.

[Top]

Previous