# Fill to Position node

The Fill to Position node uses the output of the Fill node and fills all detected areas with a greyscale color that depends on their position.

## Inputs

The Fill to Position node accepts the output of a Fill node (or a compatible output of another node) as input.

## Outputs

The Fill to Position node generates a single greyscale image map whose value is the position (on the X or Y axis) of the center of the corresponding area.

## Parameters

The Fill to Position accepts an axis parameter.

## Example images