#Equalizer APO config file

#channel
#select all channels
#Channel: all
#select first channel(front left channel)
#Channel: L
#Channel: 1
#select channel 1 and 2
#Channel: 1 2

#preamp
Preamp: -6 dB

#peaking
#Q
Filter: ON PK Fc 100 Hz Gain 0 dB Q 10
#bandwidth
Filter: ON PK Fc 100 Hz Gain -6 dB BW Oct 0.1442

#lowpass
#default Q=0.7071
Filter: ON LP Fc 100 Hz
#Q, type name with "Q"
Filter: ON LPQ Fc 100 Hz Q 0.8071

#highpass
#default Q=0.7071
Filter: ON HP Fc 100 Hz
#Q, type name with "Q"
Filter: ON HPQ Fc 100 Hz Q 0.5071

#bandpass
#default Q=0.7071
Filter: ON BP Fc 100 Hz
#Q
Filter: ON BP Fc 100 Hz Q 0.9071

#lowshelf
#default S=0.9
Filter: ON LS Fc 100 Hz Gain 4 dB
#Slope
Filter: ON LSC 12 dB Fc 100 Hz Gain -5 dB
#Q
Filter: ON LSC Fc 100 Hz Gain 3.2 dB Q 0.6708

#highshelf
#default S=0.9
Filter: ON HS Fc 100 Hz Gain -0.5 dB
#Slope
Filter: ON HSC 3.0399 dB Fc 100 Hz Gain 4 dB
#Q
Filter: ON HSC Fc 100 Hz Gain -2 dB Q 0.6071

#notch
#default Q=30
Filter: ON NO Fc 100 Hz
#Q
Filter: ON NO Fc 100 Hz Q 12.1582

#allpass
Filter: ON AP Fc 100 Hz Q 6.4397