Paper Handling

# Paper Sources

> MP tray
> 500-Sheet Lower Paper Cassette Unit A4 (EPL-6200 only)
> Manual feed slot (EPL-6200 only)

This section describes the combinations of paper sources and paper types that you can use.

## MP tray

Paper Type | Capacity | Paper Size
Plain paper | EPL-6200 Up to 250 sheets of 75 g/m2 paper (Weight: 60 to 90 g/m2, 16 to 24 lb) EPL-6200L Up to 150 sheets of 75 g/m2 paper (Weight: 60 to 90 g/m2, 16 to 24 lb) | A4, A5, B5, Letter (LT), Legal (LGL), F4, Half-Letter (HLT), Executive (EXE), ISO-B5 (IB5) Government Letter (GLT), Government Legal (GLG), Custom-size paper: 76.2 x 127.0 mm (3.0 x 5.0 in.) minimum 216.0 x 355.6 mm (8.5 x 14.0 in. maximum
Letterhead
Labels | Up to 10 sheets (Weight: 90 to 163 g/m2, 24 to 43 lb)
Thick paper
Transparencies | Up to 5 Sheets
Envelopes | Up to 10 sheets (Weight: 85 to 105 g/m2, 23 to 28 lb) | Monarch (MON), Commercial 10 (C10), DL, C6, C5, ISO-B5 (IB5)

[Top]

## 500-Sheet Lower Paper Cassette Unit A4 (EPL-6200 only)

The optional 500-Sheet Lower Paper Cassette Unit A4 gives you a second paper source in addition to the MP tray. For details on the specifications of the 500-Sheet Lower Paper Cassette Unit A4, see 500-Sheet Lower Paper Cassette Unit A4 (C12C802042) (EPL-6200 only).

[Top]

## Manual feed slot (EPL-6200 only)

The manual feed slot enables you to feed paper manually, one sheet at a time. Use the manual feed slot when you need to print on special media that you do not usually print on. By doing so, you can avoid the trouble of removing paper that is loaded in the MP tray and replacing it with the media that you want to print on. This is particularly convenient when you only need to print one sheet or very few sheets.

[Top]

Next