Setup & Maintenance / Installing and Removing Options (EPL-6200 only)

# 500-Sheet Lower Paper Cassette Unit A4

> Installing the 500-Sheet Lower Paper Cassette Unit A4
> Removing the 500-Sheet Lower Paper Cassette Unit A4

The optional 500-Sheet Lower Paper Cassette Unit A4 gives you a second paper source in addition to the MP tray. This section describes how to install and remove the cassette unit.

## Installing the 500-Sheet Lower Paper Cassette Unit A4

Follow these steps to install the optional 500-Sheet Lower Paper Cassette Unit A4:

| Turn off the printer.

| Unplug the printer's power cord from the electrical outlet and from the printer.

| Remove all interface cables from the interface connectors.

| Unpack the 500-Sheet Lower Paper Cassette Unit A4 and remove all protective materials.

| Make sure that the printer and the cassette unit are facing the same way. Lift the printer and align the pins on the cassette unit with the holes on the bottom of the printer, then lower the printer until it rests securely on the cassette unit.

| Lift off the tray cover and press down on the plate in the paper tray until it locks into position. Then insert the paper tray into the cassette unit.

| Replace the tray cover.

| Reconnect any interface cables you removed.

| Make sure that the printer's power switch is turned off before plugging the power cord into the printer and into an electrical outlet.

| Turn on the printer.

To confirm that the 500-Sheet Lower Paper Cassette Unit A4 is installed correctly, print a status sheet. See Printing a Status Sheet to print a status sheet.

To use the 500-Sheet Lower Paper Cassette Unit A4 as the paper source, be sure to choose Lower Cassette in the printer driver or Lower Cassette in the Remote Control Panel utility as the Paper Source setting.

| Note:

If your computer is running Windows Me, 98, 95, XP, 2000, or NT 4.0, you can also confirm that the 500-Sheet Lower Paper Cassette Unit A4 is correctly installed by checking the information displayed in the printer driver's Optional Settings menu.

[Top]

## Removing the 500-Sheet Lower Paper Cassette Unit A4

To remove the 500-Sheet Lower Paper Cassette Unit A4, perform the installation procedure in reverse.

[Top]

Previous | Next