Product Information / Technical Specifications

# Options and Consumables

> 500-Sheet Lower Paper Cassette Unit A4 (C12C802042) (EPL-6200 only)
> Duplex Unit (C12C802051) (EPL-6200 only)
> Memory module (EPL-6200 only)
> Developer Cartridge (S050166)
> Developer Cartridge (S050167)
> Photoconductor unit (S051099)

## 500-Sheet Lower Paper Cassette Unit A4 (C12C802042) (EPL-6200 only)

Paper size: | A4
Paper weight: | 60 to 90 g/m2 (16 to 24 lb)
Paper feed: | Automatic feed delivery system Tray capacity of up to 500 sheets (75 g/m2 or 20 lb paper)
Paper feed speed: | For the first sheet, 16 seconds or less; subsequent sheets, 20 pages per minute (at 600 dpi)
Paper types: | Plain paper, such as copier paper, and recycled paper
Power supply: | 5V/24V supplied by the printer
Dimensions and weight:
Height | 119 mm (5.4 in.)
Width | 401 mm (15.0 in.)
Depth | 438 mm (17.5 in.) including the tray
Weight | 4.0 kg (8.8 lb) including the tray
Model: | 4516*
| * This product conforms to CE marking requirements in accordance with EC Directive 89/336/EEC.

[Top]

## Duplex Unit (C12C802051) (EPL-6200 only)

Height: | 395.6 mm
Width: | 324.7 mm
Depth: | 109.3 mm
Weight: | 1.8 kg
Model: | 4517*
| * This product conforms to CE marking requirements in accordance with EC Directive 89/336/EEC.

[Top]

## Memory module (EPL-6200 only)

Make sure that the DIMM you purchase is compatible with EPSON products. For details, contact the store where you purchased this printer or the EPSON sales company.

Memory Size: | 16 MB, 32 MB, 64 MB, or 128 MB

[Top]

## Developer Cartridge (S050166)

| Note:

This developer cartridge can be used only with the EPL-6200.

Storage temperature: | 0 to 35°C (32 to 95°F)
Storage humidity: | 30 to 85% RH
Shelf life: | 18 months after production
Life: | Up to 6,000 pages under the following conditions: Letter or A4 paper, continuous printing, and 5% print ratio
Model: | 4518*
| * This product conforms to CE marking requirements in accordance with EC Directive 89/336/EEC.

[Top]

## Developer Cartridge (S050167)

Storage temperature: | 0 to 35°C (32 to 95°F)
Storage humidity: | 30 to 85% RH
Shelf life: | 18 months after production
Life: | Up to 3,000 pages under the following conditions: Letter or A4 paper, continuous printing, and 5% print ratio
Model: | 4518*
| * This product conforms to CE marking requirements in accordance with EC Directive 89/336/EEC.

| Note:

This is the developer cartridge that comes with the EPL-6200 at the time of purchase. The EPL-6200L comes with a developer cartridge that prints up to 1,500 pages.

[Top]

## Photoconductor unit (S051099)

Storage temperature: | 0 to 35 °C (32 to 95 °F)
Storage humidity: | 30 to 85% RH
Shelf life: | 18 months after production
Life: | Up to 20,000 pages under the following conditions: Letter or A4 size paper, continuous printing, 5% print ratio

| Note:

The number of pages you can print with a developer cartridge or a photoconductor unit varies depending on the type of printing. If you print a few pages at a time or print dense text exceeding the 5% print ratio, the cartridge and/or unit may print fewer pages. The 5% print ratio is equivalent to printing double-spaced standard text.

[Top]

Previous | Next