About Your Printer

# Control Panel

> Indicator lights
> Buttons (EPL-6200 only)

The EPL-6200 has six indicator lights and three buttons, while the EPL-6200L comes with two indicator lights. The indicator lights inform you of basic printer status, errors, and warnings. The buttons allow you to control a number of basic printer operations.

## Indicator lights

EPL-6200

EPL-6200L

a | Memory | Usually turns on or flashes in combination with other lights to indicate a memory-related error or warning.
b | Toner | On when the printer's developer cartridge has run out of toner. Flashes to indicate that toner is running low. If this light is flashing, have a new developer cartridge ready.
c | Paper | Turns on or flashes, and when in combination with the Error light, usually indicates a paper-related problem. On usually indicates a paper jam, while flashing usually indicates a paper-related error or warning, such as when the paper source is empty.
d | Error | On or flashes when an error is detected.
e | Ready | On when the printer is ready, indicating that the printer is ready to receive and print data. When the printer is not ready, this light is off. This light also comes on in combination with other lights to indicate error situations.
f | Data | On when data is received and stored in the print buffer (the section of memory reserved for receiving data) but not yet printed. Flashing indicates that the printer is processing data. When no data remains in the print buffer, this light is off.

For details on the errors indicated by these lights, see Status and Error Lights (EPL-6200 only).

[Top]

## Buttons (EPL-6200 only)

a | Start/Stop | Switches the printer between ready and offline status.
b | Job Cancel | Deletes the oldest print job stored in the printer. Deletes one job when pressed once. Pressing it down for more than two seconds deletes all data in the print buffer, all jobs, and all data the printer is receiving or currently printing.
c | Information | Prints a status sheet when the Error light is off and no warning is indicated. Clears the warning when a warning is indicated.

[Top]

Previous | Next