Intel® Chipset Software Installation Utility
8.1.1.1010 Production Version
Release Notes

November 8, 2006
Microsoft Windows* 2000
Microsoft Windows* XP
Microsoft Windows Server* 2003
Microsoft Vista* RTM

(and Service Packs)

DISCLAIMER: Information in this document is provided in connection with Intel® products. Intel Corporation may have patents or pending patent applications, trademarks, copyrights, or other intellectual property rights that relate to the presented subject matter. The furnishing of documents and other materials and information does not provide any license, express or implied, by estoppel or otherwise, to any such patents, trademarks, copyrights, or other intellectual property rights. Except as provided in Intel's Terms and Conditions of Sale for such products, Intel assumes no liability whatsoever, and Intel disclaims any express or implied warranty relating to sale and/or use of Intel products, including liability or warranties relating to fitness for a particular purpose, merchantability or infringement of any patent, copyright or other intellectual property right. Intel products are not intended for use in medical, life saving, life sustaining, critical control or safety systems, or in nuclear facility applications. Intel may make changes to specifications and product descriptions at any time, without notice. Contact your local Intel sales office or your distributor to obtain the latest specifications and before placing your product order.
* Intel is a trademark or registered trademark of Intel Corporation or its subsidiaries in the United States and other countries.* Other brands and names are the property of their respective owners.
Copyright © Intel Corporation 2006
Notice: The Intel® Chipset Software Installation Utility Software may contain design defects or errors described as "known issues" which may cause the product to deviate from expected performance. Current characterized known issues are documented in this update.

Revision History

Date | Driver Revision | Draft/Changes
November 8, 2006 | PV Build 8.1.1.1010 | PV Build 8.1.1.1009
October 25, 2006 | PV Build 8.1.1.1009 | Hot Fix Build 8.1.1.1005
October 11, 2006 | Hot Fix Build 8.1.1.1005 | PV Build 8.1.1.1001
May 31, 2006 | PV Build 8.1.1.1001 | Initial Release

Intel® Chipset Software Installation Utility Support

The Intel® Chipset Software Installation Utility contains support for the following Intel Chipsets:

· Intel® E7210 Chipset

· Intel® E7220 Chipset

· Intel® E7221 Chipset

· Intel® E7230 Chipset

· Intel® E7320 Chipset

· Intel® E7520 Chipset

· Intel® E7525 Chipset

· Intel® E8500 Chipset

· Intel® E8501 Chipset

· Intel® 848P Chipset

· Intel® 865G Chipset

· Intel® 865PE Chipset

· Intel® 865P Chipset

· Intel® 865GV Chipset

· Intel® 875P Chipset

· Intel® 910GE Express Chipset

· Intel® 910GL Express Chipset

· Intel® 910GML Express Chipset

· Intel® 915G Express Chipset

· Intel® 915P Express Chipset

· Intel® 915GV Express Chipset

· Intel® 915GL Express Chipset

· Intel® 915PL Express Chipset

· Intel® 915GV Express Chipset

· Intel® 915PM Express Chipset

· Intel® 915GM Express Chipset

· Intel® 915GMS Express Chipset

· Intel® 925X Express Chipset

· Intel® 925XE Express Chipset

· Intel® 940GML Chipset

· Intel® 943GML Chipset

· Intel® 945G Express Chipset

· Intel® 945GM Express Chipset

· Intel® 945GMS Express Chipset

· Intel® 945P Express Chipset

· Intel® 945PL Express Chipset

· Intel® 945PM Express Chipset

· Intel® 955X Express Chipset

· Intel® 955XM Express Chipset

· Intel® 975X Express Chipset

· Intel® 5000 Series Chipset

· Intel® 3000/3010/3100 Chipset

· Intel® Q963 Chipset

· Intel® Q965 Chipset

· Intel® P965 Chipset

· Intel® G965 Chipset

· Intel® 946GZ Chipset

· Intel® 946PL Chipset

· Intel® 946GL Chipset

Supported Operating Systems

The Intel® Chipset Software Installation Utility is validated on the following Microsoft operating systems.

1. Microsoft Windows* 2000
2. Microsoft Windows* XP
3. Microsoft Windows Server* 2003
4. Microsoft Windows Vista* RTM

New Features

Features Added in PV Build 8.1.1.1010
ID | Description
1 | Added Vista signature files for all ICH7 and ICH8 INF files
Features Added in PV Build 8.1.1.1009
ID | Description
1 | Signature files added
Features Added in Hot Fix Build 8.1.1.1005
ID | Description
1 | Added 943GML text string
Features Added in PV Build 8.1.1.1001
ID | Description
1 | Added Broadwater and Whitmore Lake DIDs and FNS including WHQL INFs

Known Issues

Known Issues in PV Build 8.1.1.1010
ID | Description
1 | When using the self extracting executable (InstallShield Package For The Web) the Vista “Program Compatibility Assistant” dialog will appear; to avoid this scenario use the zipped version.
Known Issues in PV Build 8.1.1.1009
ID | Description
1 | None
Known Issues in Hot Fix Build 8.1.1.1005
ID | Description
1 | None
Known Issues in PV Build 8.1.1.1001
ID | Description
1 | None

Issues Resolved

Issues Resolved in PV Build 8.1.1.1010
ID | Description | Affected OS's
1 | Fixed WHQL DTM failures that were caused by chipset INF files that did not have corresponding Vista signature files. | Microsoft Windows Vista
2 | Fixed Vista “Program Compatibility Assistant” dialog for showing when using the setup.exe file. | Microsoft Windows Vista
Issues Resolved in PV Build 8.1.1.1009
ID | Description |
1 | None |
Issues Resolved in Hot Fix Build 8.1.1.1005
ID | Description |
1 | None |
Issues Resolved in PV Build 8.1.1.1001
ID | Description | Affected OS's
1 | Fixed and WHQL’d the following INFs. (incorr char: 5000xzvp.inf, 945.inf, ICH8core.inf) | All

Software Sightings and/or Known Issues

ID | Information
1 | On Windows 2000 Operating system if the Intel® 82801 BA/BAM AC '97 Audio Controller device is enabled, the system may fail to enter the ACPI S3 system power state. On certain systems, the issue has been attributed to some behavior experienced with the AC '97 Audio Device driver included with Windows 2000 operating system. To address this issue install an updated device driver for the Intel® 82801 BA/BAM AC '97 Audio Controller.
2 | During the Windows setup stage; the USB keyboard and mouse may not be accessible. This is because the legacy USB driver may be inactive when Windows enters the GUI mode. There is a small window of time when it may not be possible for the system to accept user input. Since the Chipset Software Installation Utility may cause prompts during the Windows setup stage, it should be ensured that the system BIOS support for legacy USB keyboard and mouse is enabled.
3 | Older revisions of the Intel® LANDesk Software Package may cause a Device Manager warning when installed on a system after the Chipset Software Installation Utility has been executed on the system.